**ST-8 Lazer LED Light**

**Technical Specifications**

|  | | |
| --- | --- | --- |
| Voltage Range | 9-32V |  | |
| LED Life | 50,000 hours |  | |
| Optical efficiency | 88% |  | |
| Weight | 800 gr |  | |
| HIGH BEAM PERFORMANCE | | | |
| Total luminous Flux | 6944 Lm |  | |
| Number of High Output LEDs | 8 |  | |
| Power consumption | 86 Watts |  | |
| Current draw (at 14.4V) | 6 Amps |  | |
| CERTIFICATION | | | |
| High Beam | ECE R112 |  | |
| DIMENSIONS | | | |
| Width | 360 mm |  | |
| Depth | 82 mm |  | |
| Height | 72 mm |  | |
| PHOTOMETRIC DATA | | | |
| 0.25 lx line | 560 metres |  | |
| 0.5 lx line | 396 metres |  | |
| 1 lx line | 280 metres |  | |
| 3 lx line | 162 metres |  | |